
1. 9:
2. NAME = Dayne - PSK
3. Tx. Rate of Management Frame(2.4GHz) = 2.0Mbps
4. Tx. Rate of Management Frame(5GHz) = 6.0Mbps
5. Beacon Interval = 100ms
6. SSID = Dayne - PSK
7. Description =
8. Type = Standard Usage
9. Authentication = open
10. Encryption = wpa2
11. Algorithm = aes
12. Passphrase = testtest
13. FT Roaming = Disabled
14. 802.11k Neighbor report = Disabled
15. Web Authentication = Disabled
16. Authentication Server = Disabled
17. Called-Station-Id type = wlan-bssid
18. Tunnel Mode = Disabled
19. Background Scanning = Enabled
20. Max. Clients = 100
21. Isolation per AP = Disabled
22. Isolation across AP = Disabled



1. Zero-IT Activation = Disabled
2. Priority = High
3. Load Balancing = Disabled
4. Band Balancing = Disabled
5. Dynamic PSK = Disabled
6. Rate Limiting Uplink = Disabled
7. PerSSID Rate Limiting Uplink = 0
8. Rate Limiting Downlink = Disabled
9. PerSSID Rate Limiting Downlink = 0
10. Auto-Proxy configuration:
11. Status = Disabled
12. Inactivity Timeout:
13. Status = Enabled
14. Timeout = 5 Minutes
15. VLAN-ID = 1
16. Dynamic VLAN = Disabled
17. Closed System = Disabled
18. Https Redirection = Disabled
19. OFDM-Only State = Disabled
20. Multicast Filter State = Disabled
21. Directed Multicast= Enabled
22. 802.11d State = Enabled
23. Force DHCP State = Disabled
24. Force DHCP Timeout = 10
25. DHCP Option82:
26. Status = Disabled
27. Option82 sub-Option1 = Disabled
28. Option82 sub-Option2 = Disabled
29. Option82 sub-Option150 = Disabled
30. Option82 sub-Option151 = Disabled
31. Ignore unauthorized client statistic = Disabled
32. STA Info Extraction State = Enabled
33. BSS Minrate = Disabled
34. DTIM period = 1
35. Directed MC/BC Threshold = 5
36. Call Admission Control State = Disabled
37. PMK Cache Timeout= 720 minutes
38. PMK Cache for Reconnect= Enabled
39. NAS-ID Type= wlan-bssid
40. Roaming Acct-Interim-Update= Disabled
41. PAP Message Authenticator = Enabled
42. Send EAP-Failure = Disabled
43. L2/MAC = No ACLS
44. L3/L4/IP Address = No ACLS
45. L3/L4/IPv6 Address = No ACLS
46. Precedence = Default
47. Proxy ARP = Disabled
48. Device Policy = No ACLS
49. Vlan Pool = No Pools
50. Role based Access Control Policy = Disabled
51. SmartRoam = Disabled Roam-factor = 1
52. White List = No ACLS
53. URL Filtering = Disabled
54. Application Recognition & Control = Disabled
55. Apply ARC Policy = NO POLICY
56. Client Flow Data Logging = Disabled
57. Wlan Bind = all
58. Client Connection Data = Disabled
59. Transient Client Management = Disabled
60. 80211w-pmf = Disabled